Search wiring.org.co:

Libraries \ SPI

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Name |

### setBitOrder()

Examples |
    // set bit order to LSBFIRST
    SPI.setBitorder(LSBFIRST);
Description | The Serial Peripheral Interface Bus or SPI bus is a synchronous serial data link standard named by Motorola that operates in full duplex mode. Devices communicate in a master/slave mode where the master device initiates the data frame. Multiple slave devices are allowed with individual slave select (chip select) lines using a pin for each device. The setBitOrder() method sets the bit order to use for SPI communication. On Wiring v1 boards the SPI pins are: SS=24, MOSI=25, MISO=26 and SCK=27. On Wiring S board the SPI pins are: SS=20, MOSI=21, MISO=22 and SCK=23.
Syntax |
    SPI.setBitorder(bitOrder)
Parameters |

bitOrder | MSBFIRST or LSBFIRST: the bit order to use. MSBFIRST stands for most significant bit first (leftmost bit), LSBFIRST stands for less significant bit first (rightmost bit).

Returns | None
Usage | Application

Updated on July 07, 2011 11:11:43pm PDT