Search wiring.org.co:

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Name |

### noAnalogWrite()

Examples |
    ...

    noAnalogWrite(29);  // stops PWM output for pin 29

    ...
Description | The noAnalogWrite() method stops the PWM output of a PWM output pin. On Wiring v1 boards the PWM capable pins are: 29, 30, 31, 35, 36 and 37. On Wiring S board the PWM capable pins are: 4, 5, 6, 7, 19 and 20. Note: noAnalogWrite is an alias for PWMOff() command.
Syntax |
    noAnalogWrite(pin)
Parameters |

pin | int: The PWM output pin number

Returns | None
Usage | Application
Related | analogWrite() setPWMResolution() setPWMPrescale() analogRead()

Updated on July 07, 2011 11:08:43pm PDT