Search wiring.org.co:

Libraries \ Servo

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | Servo
Name |

### writeMicroseconds()

Examples |
    #include "Servo.h"

    Servo myservo;

    void setup() {
      // attaches a servo connected to pin 2
      myservo.attach(2);
    }

    void loop() {
      // sets the servo position at 0 degrees
      myservo.writeMicroseconds(544);
    }

    #include "Servo.h"

    Servo myservo;

    void setup() {
      // attaches a servo connected to pin 3
      myservo.attach(3);
    }

    void loop() {
      // sets the servo position at 180 degrees
      myservo.writeMicroseconds(2400);
    }

Description | The writeMicroseconds(ms) method sets Sets the servo pulse width in microseconds.
Syntax |
    servo.writeMicroseconds(ms)
Parameters |

servo | Any variable of type Servo
ms | int: the pulse width in microseconds

Returns | None
Usage | Application

Updated on July 07, 2011 11:11:32pm PDT