Search wiring.org.co:

Libraries \ FirmataProcessing

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | Wiring
Name |

### digitalWrite()

Examples |
    import processing.serial.*; //Import the Serial i/o and the Wiring Libraries
    import Wiring.*;
    Wiring wiring; //Create a Wiring object
    void setup() {
      println(Wiring.list()); //print the serial devices list
      //inicialized the wiring object
      wiring = new Wiring ( this, Wiring.list()[1], 57600);
      wiring.pinMode(48,Wiring.OUTPUT); //sets the pinMode
    }
    void draw() {
      if (mousePressed) {
        wiring.digitalWrite(48,Wiring.HIGH);
      }
      else {
        wiring.digitalWrite(48,Wiring.LOW);
      }
    }
Description | The digitalWrite() method sets the value of a digital output pin. Possible values are HIGH or LOW.
Syntax |
    Wiring.digitalWrite(pin, value)
Parameters |

pin | int: pin number.
value | HIGH or LOW.

Returns | None
Usage | Application

Updated on July 07, 2011 11:10:10pm PDT