Search wiring.org.co:

Libraries \ FirmataProcessing

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | Wiring
Name |

### servoWrite()

Examples |
    //Import the Serial i/o and the Wiring Libraries

    import processing.serial.*;
    import Wiring.*;
    //Create a Wiring object

    Wiring wiring;
    void setup() {
      //print the serial devices list

      println(Wiring.list());
      //inicialized the wiring object

      wiring = new Wiring ( this, Wiring.list()[1], 57600);
    }
    void draw() {
      wiring.servoWrite(0, mouseX);
    }
Description | Allows the manipulation of a servo motor. Note: To control a servo motor you don't need to defined the state of the pin using the pinMode method.
Syntax |
    Wiring.pinMode(pin, value)
Parameters |

pin | The number of the digital pin
value | The value of the position of the servo motor

Returns | None
Usage | Application

Updated on July 07, 2011 11:10:11pm PDT