Search wiring.org.co:

This example is for Wiring version 1.0 build 0100+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Wire Master Reader by Nicholas Zambetti
Demonstrates use of the Wire library Reads data from an I2C/TWI slave device Refer to the "Wire Slave Sender" example for use with this On Wiring v1 boards the SCL and SDA pins are: 0 and 1 On Wiring S board the SCL and SDA pins are: 8 and 9

    #include <Wire.h>

    void setup()
    {
      Wire.begin();        // join i2c bus (address optional for master)
      Serial.begin(9600);  // start serial for output
    }

    void loop()
    {
      Wire.requestFrom(2, 6);     // request 6 bytes from slave device #2

      while(Wire.available())     // slave may send less than requested
      {
        char c = Wire.read();  // receive a byte as character
        Serial.print(c);          // print the character
      }

      delay(500);
    }