Search wiring.org.co:

This example is for Wiring version 1.0 build 0100+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Acceleromenter ADXL335 Sparkfun breakout by BARRAGAN http://barraganstudio.com
Reads values from an accelerometer with X, Y and Z connected to analog inputs 0, 1 and 2 respectively The values are printed to the serial monitor

    int x, y, z;

    void setup()
    {
      Serial.begin(9600);      // sets the serial port to 9600
    }

    void loop()
    {
      x = analogRead(0);       // read analog input pin 0
      y = analogRead(1);       // read analog input pin 1
      z = analogRead(2);       // read analog input pin 1
      Serial.print("accelerations are x, y, z: ");
      Serial.print(x, DEC);    // print the acceleration in the X axis
      Serial.print(" ");       // prints a space between the numbers
      Serial.print(y, DEC);    // print the acceleration in the Y axis
      Serial.print(" ");       // prints a space between the numbers
      Serial.println(z, DEC);  // print the acceleration in the Z axis
      delay(100);              // wait 100ms for next reading
    }