Search wiring.org.co:

Libraries \ SoftwareSerial

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Name |

### SoftwareSerial

Examples |
    #include "SoftwareSerial.h"

    int val;
    SoftwareSerial port = SoftwareSerial(8, 9);

    void setup() {
      pinMode(8, INPUT);   // rx pin
      pinMode(9, OUTPUT);  // tx pin
      port.begin(9600);    // Start serial Serial at 9600 baud
    }

    void loop() {
      val = port.read(); // read a value and echo it
      port.print(val);
    }
Description | The SoftwareSerial class allows for creation and manipulation of software serial ports, allowing for additional serial ports besides the two hardware ports available in the Wiring I/O board. Typical baudrates are: 2400, 4800, 9600, 14400, 19200, 28800, 38400, 57600 and 115200.
Syntax |
    SoftwareSerial
Methods |

begin() |
read() |
print() |
println() |

Returns | None
Usage | Application

Updated on July 07, 2011 11:11:37pm PDT