Search wiring.org.co:

This example is for Wiring version 1.0 build 0100+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Setup and Loop.
The loop() function creates a structure in which to write programs that change with time.

    // The statements in the setup() function
    // execute once when the program begins
    void setup()
    {
      pinMode(WLED, OUTPUT); // Set the pin WLED (onboard LED) as OUTPUT
      digitalWrite(WLED, HIGH); // Set the pin WLED as HIGH (turn ON the onboard LED)
    }

    int y = 100;

    // The statements in loop() are executed until the
    // board is stopped. Each statement is executed in
    // sequence and after the last line is read, the first
    // line is executed again.
    void loop()
    {
      if (y > 0)   // Blink the LED while y > 0
      {
        digitalWrite(WLED, LOW);
        delay(100);
        digitalWrite(WLED, HIGH);
        delay(100);
      }
      y = y - 1;
    }