|  |  |  |
| --- | --- | --- |
| **To set up the Mars 2020 Clock:**   * Insert power cord into the plug in the rear of the clock (if desired, you can first remove the back panel and slip the cord through one of the slots in the lower corner of the frame, then replace panel) * Plug cord into power outlet * On initial setup, clock will automatically enter the setup routine as indicated by the clock rings turning YELLOW (after initial setup, the setup routine can be revisited by pressing the small button near the plug in the back of the clock) * After clocks turn YELLOW, join the MARS\_CLOCK WiFi network (password = Mars2020) using a mobile device or computer * Navigate to <http://192.168.4.1> in a browser (your device may take you there automatically) * Click “Configure WiFi”, select a WiFi network and enter the password * Adjust the other parameters for the clocks as desired * Press the “Save” button to save updated parameters * Navigate back to <http://192.168.4.1>, and click “Exit” to restart the clock * Enjoy!   Full rings of color on the clock faces indicate:  YELLOW — Awaiting parameter setup  PURPLE — Awaiting WiFi connection  GREEN — Awaiting time server connection  BLUE — Awaiting time sync |  |  |
|  |  |  |