Search wiring.org.co:

Libraries \ FirmataOpenframeworks

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | ofWiring
Name |

### connect()

Examples |
    void testApp::setup(){
    	wiring.connect("COM2", 57600);
    }
Description | Starts the communication with the I/O board. Note: The firmata protocole have a minimum rate of 57600 bauds.
Syntax |
    connect(port,rate)
Parameters |

port | string: the name of the port.
rate | The rate of the connection. For the Firmata Protocol the rate is 56700 bauds.

Returns | Boolean
Usage | Application

Updated on July 07, 2011 11:09:59pm PDT