Search wiring.org.co:

Libraries \ FirmataOpenframeworks

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | ofWiring
Name |

### isWiringReady()

Examples |
    void testApp::update(){
    	if ( wiring.isWiringReady()){
    		if (bSetupWiring == false){
    			setupWiring();
    			bSetupWiring = true;	// only do this once

    		}
    		// 2nd do the update of the wiring

    		updateWiring();
    	}
    }
    //--------------------------------------------------------------

    void testApp::setupWiring(){
    	wiring.sendDigitalPinMode(48, OUTPUT);
    	wiring.sendDigitalPinMode(39, INPUT);
    }
    //--------------------------------------------------------------

    void testApp::updateWiring(){
    	// update the wiring

    	wiring.update();
    }
Description | Returns true if the I/O board is ready to transfer data.
Syntax |
    isWiringReady()
Returns | Boolean
Usage | Application

Updated on July 07, 2011 11:10:02pm PDT