Search wiring.org.co:

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Name |

### digitalRead()

Examples |
    int inpin = 8;
    int outpin = 9;
    int val = 0;

    void setup() {
      pinMode(inpin, INPUT);
      pinMode(outpin, OUTPUT);
    }

    void loop() {
      val = digitalRead(inpin);
      if (val == HIGH)
      {
        digitalWrite(outpin, HIGH);
      } else {
        digitalWrite(outpin, LOW);
      }
    }
Description | The digitalRead() method reads the value of a digital input pin.
Syntax |
    digitalRead(pin)
Parameters |

pin | int: HIGH or LOW

Returns | int
Usage | Application
Related | INPUT OUTPUT HIGH LOW digitalWrite()
pinMode()

Updated on July 07, 2011 11:08:08pm PDT