Search wiring.org.co:

Libraries \ FirmataOpenframeworks

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | ofWiring
Name |

### sendDigitalPinMode()

Examples |
    void testApp::update(){
    	if ( wiring.isWiringReady()){
    		if (bSetupWiring == false){
    			setupWiring();
    			bSetupWiring = true;	// only do this once

    		}
    		// 2nd do the update of the wiring

    		updateWiring();
    	}
    }
    //--------------------------------------------------------------

    void testApp::setupWiring(){
    	wiring.sendDigitalPinMode(48, OUTPUT);
    	wiring.sendDigitalPinMode(39, INPUT);
    	wiring.sendAnalogPinReporting(0, ANALOG);
    }
    //--------------------------------------------------------------

    void testApp::updateWiring(){
    	// update the wiring

    	wiring.update();
    	cout<<wiring.getAnalog(0)<<endl;
    }
Description | Sets a digital pin as INPUT or OUTPUT mode.
Syntax |
    sendDigitalPinMode(pin,mode)
Parameters |

pin | int: The number of the pin
mode | OUTPUT or INPUT

Returns | None
Usage | Application

Updated on July 07, 2011 11:10:04pm PDT