Search wiring.org.co:

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Name |

### digitalWrite()

Examples |
    int outpin = 8;

    void setup() {
      pinMode(outpin, OUTPUT);
    }

    void loop() {
      digitalWrite(outpin, HIGH);
    }
Description | The digitalWrite() method sets the value of a digital output pin. Possible values are HIGH or LOW.
Syntax |
    digitalWrite(pin,value)
Parameters |

pin | integer value
value | HIGH or LOW

Returns | None
Usage | Application
Related | INPUT OUTPUT HIGH LOW digitalRead()
pinMode()

Updated on July 07, 2011 11:08:09pm PDT