Search wiring.org.co:

This example is for Wiring version 1.0 build 0100+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

HelloPassword by BREVIG http://alexanderbrevig.com
A demonstration of the Password library

    #include <Password.h>

    Password password = Password( "1234" );

    void setup(){
      Serial.begin(9600);

      password.append('1');   //add 1 to the guessed password
      password.append('2');   //add 2 to the guessed password
      password << '3' << '4'; //add 3 and 4 to the guessed password
      Serial.println( password.evaluate() ? "true":"false" ); //should print true, since 1234 == 1234

      password.reset(); //reset the guessed password to NULL
      Serial.println( password.evaluate() ? "true":"false" ); //should print false, since 1234 != NULL

      password.set("qwerty"); //set target password to qwerty
      Serial.println( password.is("qwerty") ? "true":"false" ); //should print true, since qwerty == qwerty
      Serial.println( password == "qwirty" ? "true":"false" ); //should print false, since qwerty != qwirty
    }

    void loop(){/*nothing to loop*/}