Search wiring.org.co:

Libraries \ FirmataProcessing

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | Wiring
Name |

### list()

Examples |
    //Import the Serial i/o and the Wiring Libraries
    import processing.serial.*;
    import Wiring.*;
    //Create a Wiring object
    Wiring wiring;
    void setup() {
      //print the serial devices list
      println(Wiring.list());
      //inicialized the wiring object
      wiring = new Wiring ( this, Wiring.list()[1], 57600);
      //sets the pinMode
      wiring.pinMode(48,Wiring.OUTPUT);
    }
    void draw() {
      //.........
    }
Description | The list() method prints in the Processing console a list of all available serial port, use println() to acces to this information.
Syntax |
    Wiring.list()
Returns | None
Usage | Application

Updated on July 07, 2011 11:10:10pm PDT