Search wiring.org.co:

Libraries \ Password

Reference for Wiring version 1.0 Build 0100+ If you have a previous version, use the reference included with your software. If see any errors or have any comments, let us know.

Class | Password
Name |

### reset()

Examples |
    #include <Password.h>

    Password password = Password( "1234" );

    void setup(){
      Serial.begin(9600);

      password.append('1');   //add 1 to the guessed password
      password.append('2');   //add 2 to the guessed password
      password << '3' << '4'; //add 3 and 4 to the guessed password
      //should print true, since 1234 == 1234
      Serial.println( password.evaluate() ? "true":"false" );

      password.reset(); //reset the guessed password to NULL
      //should print false, since 1234 != NULL
      Serial.println( password.evaluate() ? "true":"false" );

      password.set("qwerty"); //set target password to qwerty
      //should print true, since qwerty == qwerty
      Serial.println( password.is("qwerty") ? "true":"false" );
      //should print false, since qwerty != qwirty
      Serial.println( password == "qwirty" ? "true":"false" );
    }

    void loop(){/*nothing to loop*/}
Description | Reset the guess.
Syntax |
    reset()
Returns | None
Usage | Application

Updated on July 07, 2011 11:11:20pm PDT